UPLINK

EPON OLT

Layer3 version

Series Software Release Notes

About This Document

This document provides a general description of the release and its new features. It also describes additions or changes, resolved issues, and any relevant open issues by the release.

|  |  |
| --- | --- |
| version | V2.03.46 |
| date | 2018-04-26 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add dhcp-snooping binding rapid-refresh. |
| 2 | Add command: show task |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.45 |
| date | 2018-04-01 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | The Web Logo can be downloaded into olt by tftp,  the logo file is 200 x 80  download tftp web-logo <filename> <A.B.C.D>  erase web-logo, erase the web logo file  show web-logo |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.44 |
| date | 2018-03-27 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Olt records the mac conflict information when there is a event of the mac conflict, doesn’t add the onu into the black list |
| 2 | Fix a bug in oun vlan web page |
| 3 | Add core\_ip web logo  set web log core\_ip |

|  |  |
| --- | --- |
| version | V2.03.43 |
| date | 2018-02-27 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Support the authentication between the olt and onu |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.42 |
| date | 2018-02-23 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add the olt provider information ad web page for dbc |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.42 |
| date | 2018-01-20 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add a command for the loopback mode configuration  loopback detect enable uplink|pon|all |
| 2 | Add a command to select loopback check for each port  loopback [enable|diable] |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.41 |
| date | 2018-01-05 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | The olt will shutdown the pon port when there is a onu, which has a loopback event. |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.40 |
| date | 2017-12-26 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | the loopback is in onu mode, not in pon port mode |
| 2 | When the startup is time out, the aux will be opened, the initialized pon ports will be in work mode. |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.39 |
| date | 2017-12-12 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add a command to select a web page logo at the debug mode  epon-olt(debug-mode)# set web logo none  this is a command to select a neutral web page logo |
| 2 | Fix the bug of the de-register onu, this will cause the onu invalid. |
| 3 | The olt will close the pon port when there is a loopback between a uplink and a pon |

|  |  |
| --- | --- |
| version | V2.03.38 |
| date | 2017-12-11 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | The version for CS8022 upgrade to V4.2.7.61 |
| 2 | Don’t delete the onu configurations when the olt fails to send the configurations to the onu |
| 3 | Add a cli command to query the failed download configurations  epon-olt(config-pon-0/1)# show running-config error onu |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.37 |
| date | 2017-11-28 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Fix a bug for ntp,it causes cpu usage uo to 100％ |
| 2 | Add a command for pon whether to offline the onu when the system cpu receives a pon los event.  pon down clear record [enable|disable] |
| 3 | Fix a questionable ways when a onu is time out |

|  |  |
| --- | --- |
| version | V2.03.36 |
| date | 2017-11-09 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Change the default web logout time to ten minutes  web login timeout <1-30>  show web login timeout |
| 2 | Add the command to show all interface’s information  show interface breif |
| 3 | Add the onu’s distance information in onu status command  show onu status all |

|  |  |
| --- | --- |
| version | V2.03.35 |
| date | 2017-10-17 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Support neuter vendor and module id |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.34 |
| date | 2017-10-17 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add user’s authority level in web management |
| 2 | Add a command to check the olt type  epon-olt(debug-mode)# show global information |
| 3 |  |

|  |  |
| --- | --- |
| version | V2.03.33 |
| date | 2017-10-11 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Support V.SOL web logo |
| 2 | Fixed 10G interface information error |
| 3 |  |
| 4 |  |

|  |  |
| --- | --- |
| version | V2.03.32 |
| date | 2017-08-24 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add loopback detection, the following is the configuration commands:  loopback detect enable  no loopback detect  loopback mode [only-alarm|manual-recovery]  loopback aging-time <30-3600>  show loopback detect  onu black-mac-auth del <mac> or onu black-mac-auth clean |
|  |  |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.31 |
| date | 2017-08-04 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add allowed functions for web ,snmp and telnet management ip  login-access-list [enable|disable]  login-access-list [permit|deny] [telnet|web|snmp] <A.B.C.D> <A.B.C.D>  the permit priority is higher than the deny priority |
| 2 | Support the third party catv control  onu catv packet [cdcom|bdcom|ftcom] |
| 3 | Support dude monitor software |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.30 |
| date | 2017-06-16 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Fix the bug for 10G port, cann’t ping the vlan interface ip from the 10G port |
| 2 | Update the web server |
| 3 | Fix the ping program statistic issue |
| 4 |  |

|  |  |
| --- | --- |
| version | V2.03.29 |
| date | 2017-05-09 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | The onu will quit when it’s oam registration is time out |
| 2 | Fix the issue of onu reboot when olt snmp gets onu’s optical power value |
| 3 | Add a command for changing http port  httpd port <1-65535> |
| 4 |  |

|  |  |
| --- | --- |
| version | V2.03.28 |
| date | 2017-04-13 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Reduce the cpu utilization by optimizing application code |
| 2 | Add mac address limit for a llid under a pon interface  onu <1-65535> [mac-limit] <0-16383> |
| 3 |  |
| 4 |  |

|  |  |
| --- | --- |
| version | V2.03.27 |
| date | 2017-03-30 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add an extend command for non standard oam onu  **onu ext-support check [enable|disable]**, default is enable |
| 2 | Add some CLI command to show olt or onu’s information based on a special interface |
| 3 | Support the olt V1600D16 |
| 4 | Fix the web disconnect issue |

|  |  |
| --- | --- |
| version | V2.03.26 |
| date | 2017-03-11 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add the auto-bind profile for onus in a pon port  **onu [auto-bind] profile [dba|srv|voip|alarm] id <0-32767>**  **show onu [auto-bind] [profile\_id]** |
| 2 | Find the host mac position |
| 3 | Can show the time of onu register, deregister and running |
| 4 | Support the onu with a invalid source mac |
| 5 | Support the third party tool software such as MRTG and syslog |
| 6 | Provide onu’s informations about register, deregister, the reason of deregister and running time |

|  |  |
| --- | --- |
| version | V2.03.25 |
| date | 2017-02-08 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Fix a bugs for a reserved source mac address |
| 2 | Remove the Broadcom chip information |

|  |  |
| --- | --- |
| version | V2.03.24 |
| date | 2017-01-18 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Fix some bugs from new web test |
| 2 | Fixed a null pointer inV2.03.22 and V2.03.23 |

|  |  |
| --- | --- |
| version | V2.03.23 |
| date | 2016-12-07 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add dhcp server management for onu |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.22 |
| date | 2016-12-07 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add dhcp server management for onu |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.21 |
| date | 2016-11-28 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | The new style web management |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.20 |
| date | 2016-11-22 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | The WAN connect is not effective at the first time |
| 2 | Fixed a wrong snmp object id |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.19 |
| date | 2016-10-20 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add WAN and WiFi management on WEB for V2801HW |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.18 |
| date | 2016-10-10 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Improve the sfp port auto-negotiation for 1000M |
| 2 | Modify the onu type name according to it’s capability |
| 3 | Improve some system cmd for telnet operation |
| 4 | Improve the vlan interface ip revise operation |
| 5 | Add the force auto-update for onu firmware |

|  |  |
| --- | --- |
| version | V2.03.17 |
| date | 2016-09-19 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add the function to show onu mac address under a pon port |
| 2 | Add a turn on-off for a pon port to check whether a onu is laser on or off automatically |
| 3 | Improve the oam process for the fault that the pon chip doesn’t send oam packet to cpu |
| 4 | Add the c-date catv module control |

|  |  |
| --- | --- |
| version | V2.03.16 |
| date | 2016-08-31 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Adapt other company’s onu when it cann’t finish the  Oam version autonegation ,otherwise it will be in busy state |
| 2 | Add onu registration protection mechanism, Olt will restart onu registration when it is over five minutes |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.15 |
| date | 2016-08-25 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | modify some web display information errors |
|  |  |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.15 |
| date | 2016-08-12 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Adapt the wrong version number for V2801HW |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.15 |
| date | 2016-08-9 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Improve the onu response when a onu return a value 0x0,change it to 0x86,it means that the attribute or the action is invalid. |
| 2 | Add user management in web |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.14 |
| date | 2016-08-01 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Change the time of the onu bandwidth assignment, when a onu is authenticated, the olt will assign the bandwidth for it |
| 2 | Improve the oam communication mechanism |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.13 |
| date | 2016-07-28 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add web management |
| 2 | Add update the onu firmware automatically |
| 3 | Fix olt oam process when onu responses a wrong oam |
| 4 | Fix a bug for saveing default user password issue |

|  |  |
| --- | --- |
| version | V2.03.12 |
| date | 2016-05-11 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Fixed a bug for onu mac authentication |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.11 |
| date | 2016-04-29 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add a state for ems system when a onu finished it’s register |
| 2 | Fixed a CLI login bug for character ‘!’,you can go into config mode when you input the character ‘!’ |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.10 |
| date | 2016-04-15 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | improve onu register process because this problem will cause the OLT does not respond to onu |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.09 |
| date | 2016-03-29 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Fixed a bug for deleting a onu operation, the onu can not register if do not reboot the olt |
| 2 | Add a command to show all onu’s receive power in a pon |
| 3 | the acl rule can be used in Multiple ports |

|  |  |
| --- | --- |
| version | V2.03.08 |
| date | 2016-03-23 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Fixed some operations for ems management |
| 2 | Add olt serial number and mac authentication |

|  |  |
| --- | --- |
| version | V2.03.07 |
| date | 2016-03-01 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add ONU communication for the same pon port |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.06 |
| date | 2016-02-26 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add private oam for CATV,WIFI management |
| 2 | Add DHCP Server, DHCP Relay, DHCP SNOOPING |

|  |  |
| --- | --- |
| version | V2.03.05 |
| date | 2016-01-13 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Change l2ftp timeout from 15s to 30s to avoid re-sending image block |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.04 |
| date | 2016-01-4 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Disable automatic conntrack |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.03 |
| date | 2015-12-30 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Fix some issues for EMS service profile configuration |
|  |  |

|  |  |
| --- | --- |
| version | V2.03.01 |
| date | 2015-12-21 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add OLT type hardware identification,so D2,D4,D8 will use the same firmware |
|  |  |

|  |  |
| --- | --- |
| version | V1.03.49 |
| date | 2015-12-14 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Fix a issue for HG323UE register link lose |
| 2 | Use olt type string to identify what type of olt the olt is |
| 3 |  |

|  |  |
| --- | --- |
| version | V1.03.45 |
| date | 2015-11-30 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Change aux port bandwidth from 5M to 10M |
| 2 | Fix a issue for default onu type, it cann’t identify the known onu types |
| 3 | Cancel the aux brandwidth limit for aux download issue |

|  |  |
| --- | --- |
| version | V1.03.43 |
| date | 2015-11-25 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Fixed a upload configure file to tftp server issue |
| 2 | Improve the ctc extend oam discovery process |
| 3 | Add default onu type for 1GE,4GE,4FE,8FE |

|  |  |
| --- | --- |
| version | V1.03.42 |
| date | 2015-11-12 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Fixed a onu port issue for snmp process |
| 2 | Fixed a onu multicast vlan strip issue for snmp process |
| 3 | Add a re-transmission mechanism during the period of onu discovery |

|  |  |
| --- | --- |
| version | V1.03.41 |
| date | 2015-11-3 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add the function to check the vlan ip address with the aux interface’s address whether or not the same |
| 2 | Save the ip route 0.0.0.0/0 configuration |
| 3 | Add the gateway for aux interface |
| 4 | Delete a port by switchport hybrid vlan 1 untagged,  Then save and reboot, the port will not has switchport hybrid vlan 1 untagged configuration |