jeśli soft w OLT jest starszy niż V2.03.57R należy najpierw przeprowadzić aktualizację do tej wersji:

1. rozpakowujemy archiwum V2.03.57R.zip i wgrywamy najpierw plik UBI_V2.03.57R.ubi i rebootujemy OLT, następnie wgryamy plik IMG_V2.03.57R.img i tu również po wgraniu robimy reboot
2. jeśli soft jest w wersji .57R lub nowszej ale nie ma funkcjonalności IPv6 to najpierw wgrywamy V2.03.57R_IPv6_ALLinONE.ubi
3. wgrywamy pliki z najnowszej wersji przy czym OLT rebootujemy dopiero po wrzuceniu obu
gotowe



becasue OLT provious version doesn't support IPv6, need to upgrade the intermediate version and then upgrade the latest versioin. if OLT already supports IPv6, upgrade the latest version directly.

upgrade steps:

1. if OLT current version is less than V2.03.57R, please upgrade to V2.03.57R first.
  (1)uncompress the fileV2.03.57R.zip, upgrade UBI_V2.03.57R.ubi and reboot OLT. then upgrade IMG_V2.03.57R.img and reboot OLT again.
  (2)ugprade V2.03.57R_IPv6_ALLinONE.ubi and reboot OLT.

2. if OLT current version is or over V2.03.57R, please upgrade V2.03.57R_IPv6_ALLinONE.ubi. then reboot OLT again.

3. after upgraded to V2.03.57R, please upgrade the latest version.(after upgraded both files ubi and img, reboot OLT)