V1600G Series Software Release Notes

v-solution

**About This Document**

This Document provides a general description of the release and its new features. It also describes additions or changes, resolved issues, and any relevant open issues by the release.

|  |  |
| --- | --- |
| Version | V1.8.5 |
| Date | 20180428 |
|  | |
| Item | The description of the release and its features. |
| 1. | Modify WAN configuration of WEB. |
| 2. | Add Function: private wifi/voip/dhcp server/misc, include CLI/WEB/EMS |
| 3. | Fix bug: some device will be failed while using untag or vlan 1 on ONU. |
| 4. | Fix bug: line profile failed. |
| 5. | Fix bug: web description or name invalid check. |
| 6. | Fix bug: system failed while modifying PPPoE’s WAN connection. |

|  |  |
| --- | --- |
| Version | V1.8.4 |
| Date | 20180206 |
|  | |
| Item | The description of the release and its features. |
| 1. | Fix bug: modify default dba profile will cause segmentation fault. |
| 2. | Fix bug: show upgrade onu-version will cause segmentation fault. |
| 3. | Add function: olt loopback detect. |
| 4. | Finish function: private protocol --WAN\VOIP configuration. |
| 5. | Add function: after boot up, check once DDR test result. If DDR test error, keep SYS led state. |
| 6. | Fix bug: profile name too long will cause segmentation fault. |

|  |  |
| --- | --- |
| Version | V1.8.3 |
| Date | 20171220 |
|  | |
| Item | The description of the release and its features. |
| 1. | Add function: show sys license command and WEB’s license show. |
| 2. | Add function: change web logo by command. |
| 3. | Add function: some private protocol |
| 4. |  |
| 5. |  |

|  |  |
| --- | --- |
| Version | V1.8.2 GOIP |
| Date | 20171129 |
|  | |
| Item | The description of the release and its features. |
| 1. | Add function: onu port loopdetect configuration/ alarm log. |
| 2. |  |
| 3. |  |
| 4. |  |
| 5. |  |

|  |  |
| --- | --- |
| Version | V1.8.1 |
| Date | 20171120 |
|  | |
| Item | The description of the release and its features. |
| 1. | Add function: onu main/standy software verion display on “onu detail info” |
| 2. | Add function: onu model display on “onu info” |
| 3. | Fix bug: configuration save failed while description string has space. |
| 4. | Add function: Add range vlans from web. |
| 5. | Changed: led flash mode of uplink port. Fiber: flash led while rx/tx packet. Copper: active led flash more regular. |

|  |  |
| --- | --- |
| Version | V1.7 |
| Date | 20171025 |
|  | |
| Item | The description of the release and its features. |
| 1. | Fix bug: Enable the auto-learn function on web, it still display ‘disable’ after refresh. |
| 2. | Fix bug: Incorrect onu list display on web when using ‘sn+pw’ or ‘loid+pw’ auth method. |

|  |  |
| --- | --- |
| Version | V1.6 |
| Date | 20171021 |
|  | |
| Item | The description of the release and its features. |
| 1. | Add function: onu search |
| 2. | Add function: abort onu upgrading. |
| 3. | Add function: delete onu firmware file from web. |
| 4. | Add function: omci debug. |
| 5. | Add function: catv operation on WEB. |
| 6. | Modify display: Automatic discovery onu on WEB. |
| 7. | Add function: auto get a free onu id on ‘onu add’ WEB. |
| 8. | Fix bug: auto learn function, default-onu-type not per PON, all PON share the same one. |
|  |  |

|  |  |
| --- | --- |
| Version | V1.5 |
| Date | 20170927 |
|  | |
| Item | The description of the release and its features. |
| 1. | Fix bug: while upgrading onu，refresh web may cause device reboot. |
| 2. | Add function: show onu distance |
| 3. | Add function: license alarm. |
| 4. | Add function: onu search(only cli) |
| 5. | Add function: abort onu upgrading. |
|  |  |