Instrukcja aktualizacji:

Jeśli OLT nie ma firmware w wersji 1.9.7 należy najpierw zaktualizować OLT używając pliku upgrade_V1.9.7R_ipv4.ubi i zrobić reboot. Następnie użyć pliku upgrade_V1.9.7R_all_ipv6.ubi i ponownie zrobić reboot po aktualizacji. Po tej operacji aktualizujemy urządzenie za pomocą softu v2.0.3R_20191010_tar_h.ubi

Jeśli OLT ma wersję 1.9.7 należy najpierw zaktualizować go używając pliku upgrade_V1.9.7R_all_ipv6.ubi a po reboocie wrzucamy v2.0.3R_20191010_tar_h.ubi

Jeśli OLT posiada soft nowszy od 1.9.7 ale nie wspiera IPv6 to najpierw aktualizujemy go za pomocą pliku upgrade_V1.9.7R_all_ipv6.ubi a po reboocie wrzucamy v2.0.3R_20191010_tar_h.ubi


English:
1.Because of the OLT firmware which less than V1.9.7R not support change IPv4 to IPv6(via upgrade IPv6 OLT firmware). So pls upgrade the Intermediate version to help to change IPv4 to IPv6. There are the steps :

a) if OLT current firmware less than V1.9.7R, Upgrade upgrade_V1.9.7R_ipv4.ubi and reboot olt. when starting up then Upgrade upgrade_V1.9.7R_all_ipv6.ubi and reboot olt.

b)if OLT current firmware is or over V1.9.7R and already support IPv6, pls upgrade any IPv6 firmware provided by manufacturer directly.

c)if OLT current firmware is or over V1.9.7R but not support IPv6, pls upgrade upgrade_V1.9.7R_all_ipv6.ubi or any ALLinONE IPv6 firmware provided by manufacturer.


2.Version Information:
IPv6 OLT firmware including bootˇ˘Kernal and APP files. There are the firmware version in the following:

Boot: 
U-Boot 2018.08v1.1 (Aug 22 2018 - 09:49:40)

Kernal:
Linux version 3.6.5 (samson@ubuntu) (gcc version 4.7.2 (Broadcom Linux) ) #116 SMP Fri Apr 19 14:55:04 CST 2019

APP:
  Hardware Version:            eight gpon olt platform
  Software Version:            V1.9.7R
  Software Created Time:       Wed, 22 May 2019 11:41:33 +0800
