Uplink EPON OLT L2 Series Software Release Notes

UPLINK

About This Document

This document provides a general description of the release and its new features. It also describes additions or changes, resolved issues, and any relevant open issues by the release.

|  |  |
| --- | --- |
| version | V1.01.48 |
| date | 2019-04-30 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Support the limit of onu number and running time. |
| 2 |  |
| 3 |  |

|  |  |
| --- | --- |
| version | V1.01.46 |
| date | 2018-11-16 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Improve the snmp access traffic operation, this operation will result in  the cpu state of 100 percent utilization rate |
| 2 |  |
| 3 |  |

|  |  |
| --- | --- |
| version | V1.01.45 |
| date | 2018-09-20 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | The web supports English and chinese |
| 2 | Improve the snmp access traffic operation, this operation will result in  the cpu state of 100 percent utilization rate |
| 3 | Support shutdown for uplink port1 and port2 |

|  |  |
| --- | --- |
| version | V1.01.42 |
| date | 2018-05-17 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | The Web Logo can be downloaded into olt by tftp,  the logo file is 200 x 80  download tftp web-logo <filename> <A.B.C.D>  erase web-logo, erase the web logo file  show web-logo |
| 2 | Fix a bug for the running time, the running will be reset to zero when you set the date and time |
| 3 | Improve the snmp access traffic operation, this operation will result in  the cpu state of 100 percent utilization rate |
|  |  |

|  |  |
| --- | --- |
| version | V1.01.41 |
| date | 2018-01-23 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add a command to select a web page logo at the debug mode  epon-olt(debug-mode)# set web logo none  this is a command to select a neutral web page logo |
|  |  |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V1.01.40 |
| date | 2017-10-23 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add user’s authority level in web management |
| 2 | Support neuter vendor and module id |
|  |  |

|  |  |
| --- | --- |
| version | V1.01.39 |
| date | 2017-10-16 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Remove the default dns server 192.168.2.1 |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V1.01.38 |
| date | 2017-08-30 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add loopback detection between ouns |
|  |  |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V1.01.37 |
| date | 2017-08-14 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add the login access control for telnet ,web and snmp |
|  |  |
|  |  |
|  |  |

|  |  |
| --- | --- |
| version | V1.01.36 |
| date | 2017-08-11 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Fix the ping program statistic issue |
| 2 | Fix the web disconnect issue |
| 3 | Change the realtek source mac address to cpu mac address for hardware packets |
| 4 | Add the isolation between the CS8022 and aux port |

|  |  |
| --- | --- |
| version | V1.01.35 |
| date | 2017-05-22 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Fix the configuration saving for P2P |
| 2 | Add public snmp mib support for the third software |
| 3 |  |
| 4 |  |

|  |  |
| --- | --- |
| version | V1.01.34 |
| date | 2017-04-14 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add mac address limit for a llid under a pon interface  onu <1-65535> [mac-limit] <0-16383> |
| 2 |  |
| 3 |  |
| 4 |  |

|  |  |
| --- | --- |
| version | V1.01.33 |
| date | 2017-04-05 |

|  |  |
| --- | --- |
| item | The description of the release and its new features |
| 1 | Add some CLI command to show olt or onu’s information based on a special interface |
| 2 | Find the host mac position |
| 3 | Can show the time of onu register, deregister and running |
| 4 | Support the onu with a invalid source mac |
| 5 | Support the third party tool software such as MRTG and syslog |
| 6 | Provide onu’s informations about register, deregister, the reason of deregister and running time |